# Connect your Itron Gas Volume Converter CORUS (PTZ) to Wattics

Written by Antonio Ruzzelli
Updated over a week ago

Are you ready for energy savings? Enable our cloud-based energy analytics and dashboard for your gas meter readings, to discover, measure and verify savings in the premises you manage.

The Itron Gas Volume Converter CORUS (PTZ) is the industry-leading device to correct gas readings according to pressure, temperature and compressibility factor. You can now connect your CORUS to Wattics via our Octopus gateway in a few steps.

## 1 Configure your CORUS Pulse Outputs

The CORUS features a low frequency (LF) input used to meter unconverted volumes. That LF input can be associated to any gas meter with an electrically compliant interface: 

- Dry contact

- Static relay

- Open collector or open drain output

The CORUS then features two on/off outputs that can be each configured as: 

- unconverted volume pulse output

- converted volume pulse output

Both pulse outputs are individually characterized by a pulse weight that can be configured to any value greater than or equal to the input pulse weight among 0.001 m3/pulse, 0.01 m3/pulse, 0.1 m3/pulse, 1 m3/pulse, 10 m3/pulse, 100 m3/pulse. The outputs generate a pulse every time the corresponding (unconverted or converted) index gets increased by a value equal to the selected output pulse weight. The closing time of the volume pulse outputs can also be programmed (default value is 250ms).

Check the Itron’s user manual to wire your gas meter to the CORUS device and to configure your unconverted and converted volume pulse outputs. Installation and program procedures must be carried out and inspected by qualified personnel. Qualified personnel are those who, based on their training and experience, are capable of identifying risks and avoiding potential hazards when working with this product.

## 2 Wire your CORUS Pulse Outputs to the Octopus Gateway

`Make sure that all devices are powered off before any wiring is done.`
The Octopus gateway is a Modbus data logger that comes with 6 x digital inputs, meaning that up to 6 pulses outputs can be counted, logged and communicated to Wattics dashboard. You can connect the pulse outputs from your CORUS to the Octopus Gateway in any available input. You may have a signal barrier in between to separate the safe zone from the hazardous zone.

1. Power the Octopus and CORUS off
2. Connect the Octopus 24VDC V+ line to the Corus’ OUT1-/OUT2- (J5.6/J5.8) lines
3. Connect the CORUS OUT1+/OUT2+ (J5.5/J5.7) pulse outputs to two of the Octopus digital input lines
4. Power up the Octopus

## 3 Configure your Octopus Gateway

Once the CORUS pulse outputs are wired, the Octopus device must be configured to count, log and show measurements on your Wattics Energy Management Dashboard. You must follow the instructions below:

http://docs.wattics.com/2016/04/08/configuring-your-wattics-octopus-with-the-octopus-software-tool/

Once the configuration is completed and your data points are registered and subscribed to Wattics, you will receive access to your Wattics dashboard, and from then on will be able to log in to your Wattics Dashboard at http://dash.wattics.com to start analyzing your gas meter readings.

+353 (0)1415 1242 | info@wattics.com | Contact us

Download PDF

- About

- Latest Posts

## Anthony Schoofs

Chief Technical Officer at Wattics

Anthony drives Wattics' innovation on energy efficiency for industrial and grid environments. Anthony is also behind WSNbuzz.com, a blog covering technology advances within the smart grid and IoT markets, and was listed in 2011 amongst the top 100 IoT thinkers. Anthony was recently awarded the Globe Sustainability Research Award for his contribution to advancing knowledge on sustainability.

### Latest posts by Anthony Schoofs (see all)

- Export your Wattics data to Tableau business intelligence software - December 8, 2017

- Connect your Schneider PowerLogic PM8000 meter to Wattics with the Obvius AcquiSuite EMB A8810 Data Acquisition Server - December 7, 2017

- Connect your EIG Nexus 1500 meter to Wattics with the Obvius AcquiSuite EMB A8810 Data Acquisition Server - December 7, 2017

Did this answer your question?