# Connect your Rainforest Eagle Energy Gateway to Wattics

Written by Antonio Ruzzelli
Updated over a week ago

Are you ready for energy savings? Enable our cloud-based energy analytics and dashboard for your Rainforest Eagle Energy Gateway, to discover, measure and verify savings in the premises you manage.

It is assumed that the Eagle Energy Gateway already collects data from your meter(s). If not, read and understand Rainforest manuals for installing, operating, or maintaining your Eagle Energy Gateway. Installation and program procedures must be carried out and inspected by qualified personnel. Qualified personnel are those who, based on their training and experience, are capable of identifying risks and avoiding potential hazards when working with this product.

### Step 1: Register your data logger and data points with Wattics

Register your Eagle Energy gateway

You will need to provide the MAC address of your Eagle Gateway, which you can find underneath the device.

One of our agents will contact you to set up your monthly subscription fee and give you access to the Wattics dashboard.

### Step 2: Configure your Eagle Gateway

Access your Eagle’s user interface via rainforestcloud.com (or via the .local web address found underneath the device). Enter your credentials to access the Web Viewer and then go to Settings.

You are now ready to set up your Eagle Gateway to send data to Wattics. Expand the Cloud status bar to bring up the Cloud sub-page.

If Wattics appears as a Provider, please select it from the drop-down menu.

Otherwise, add Wattics as a provider through the “add cloud” + icon at the bottom left. When prompted, please enter the information below:

- Provider: Wattics Ltd

- URL: http://rainforest.wattics.com/eagles/data_points

Click “Add Cloud” button to save Wattics as your new Cloud Provider.

Finally, click on “Set Cloud” to start data upload to Wattics. Your data will now be sent to Wattics, log in to your dashboard and get started!

### You don’t have yet a Rainforest Eagle Energy Gateway?

Contact us if you would like to receive technical and pricing information. The Rainforest gateway reads energy measurements from your ZigBee Smart meter, and pushes interval energy use data to Wattics via your Ethernet or WiFi network. You must check that the utility in your area supports the Rainforest Eagle before enabling Wattics.

List of supported utilities

+353 (0)1415 1242 | info@wattics.com | Contact us

Download PDF

- About

- Latest Posts

## Anthony Schoofs

Chief Technical Officer at Wattics

Anthony drives Wattics' innovation on energy efficiency for industrial and grid environments. Anthony is also behind WSNbuzz.com, a blog covering technology advances within the smart grid and IoT markets, and was listed in 2011 amongst the top 100 IoT thinkers. Anthony was recently awarded the Globe Sustainability Research Award for his contribution to advancing knowledge on sustainability.

### Latest posts by Anthony Schoofs (see all)

- Export your Wattics data to Tableau business intelligence software - December 8, 2017

- Connect your Schneider PowerLogic PM8000 meter to Wattics with the Obvius AcquiSuite EMB A8810 Data Acquisition Server - December 7, 2017

- Connect your EIG Nexus 1500 meter to Wattics with the Obvius AcquiSuite EMB A8810 Data Acquisition Server - December 7, 2017

Did this answer your question?